This circuit is a Schmitt Trigger, a type of comparator, built using a 555 timer chip for some reason. It measures the input to see if it is above or below a certain threshold. The threshold varies to make it less likely that the output will switch rapidly back and forth due to a noisy input near the threshold.

This circuit uses the fact that a 555 output goes high when the trigger input goes below 1/3 Vin, and the output goes low when the threshold input goes above 2/3 Vin.

Next: 555 Missing Pulse Detector

Previous: 555 Pulse Width Modulator

Index

Simulator Home

java@falstad.com
Generated Wed Dec 7 2016