This circuit is a 2-to-1 multiplexer. It selects one of two inputs (based on the select input at the bottom right) and outputs it at the bottom. It uses two tri-state buffers; the implementation of each buffer is shown in full. When the select input is low, input 1 is used. The buffer on the left is switched on, and the buffer on the right is put in a high-impedance state where it does not have any effect on the output. When select input is high, input 2 is used.

Next: Majority Logic

Previous: 1-of-4 Decoder

Index

Simulator Home

java@falstad.com
Generated Wed Dec 7 2016